	[bookmark: _GoBack]       Client's Laminated Laying Hen Cage Quotation in Bangladesh

	Party A: China Henan Yaxuan Machinery Equipment Manufacturing Co.
	Quotation date 2024/10/10

	Party B: Client in Bangladesh
	

	Equipment type: 4 rows of five-layer cages for laying hens
	120/60/43

	Chicken house size
	Length of chicken house
	76.2
	Width of chicken house
	12.2
	Height of chicken house
	4.85
	work unit
	meter (classifier)

	Equipment Specifications
	storey
	columns
	Chickens per door
	Per assembly
quantity of chickens
	Number of cages per row
	Total number of groups
	Standardized loading 
	Chicken area (cm²/feather)

	Equipment data
	5
	4
	8
	160
	56
	224
	35840
	450

	serial number
	Product name and specification
	quantities
	work unit (one's workplace)
	Unit price (RMB)
	Subtotal (dollars)
	photograph
	note

	One、
	Cage system

	1
	five-layer cage netting
	224
	organize
	1530
	342720
	[image: ]
	Cage frame material zinc aluminum magnesium 2.0 thick, combined cage frame without welding, cage mesh hot galvanized wire, beautiful and corrosion-resistant, stamping molding flat bottom, plate thickness ≥ 1.0 ㎜; 2.4 m/root; trough support hot dipped galvanized, plate thickness ≥ 1.0 ㎜, bolts fixed to the cage frame, stepping on the use of firm.

	2
	Five-layer steel cage frame
	224
	organize
	
	
	
	

	3
	Galvanized sheet metal egg stopper
	224
	organize
	
	
	
	

	4
	five-tier trough
	224
	organize
	
	
	
	Hot-dip galvanized, 10/group cage doors with cross sliding doors

	5
	Trough Tray
	224
	organize
	
	
	
	

	6
	water dispenser
	224
	bend 
	
	
	
	Square hose, conical drinker with V-shaped trough better reduces dripping and makes chicken manure drier

	7
	Plumbing V-Sink
	224
	organize
	
	
	
	

	8
	doser
	2
	bend 
	2400
	4800
	
	Dosu doser with filter

	Total cage netting system：
	347520
	
	（RMB）

	two、
	Feeding system

	1
	Driving feeder
	4
	bend 
	10500
	42000
	[image: ]
	The hopper is made of zinc-aluminum-magnesium plate, the Taili motor is 0.75 kW, the speed ratio is 1:80, and each hopper is equipped with one material leveler made of hot-dip galvanized cold-rolled steel plate 3.0 and two return devices.

	2
	Traction devices and accessories
	
	
	
	
	
	Including 304 steel wire rope and hot dip galvanized bracket

	3
	Car guide rail
	
	
	
	
	
	3.0 Hot dip galvanized square tube

	4
	Horizontal feeding device
	
	
	
	
	
	Φ140MM galvanized pipe indoor feeding device, auger motor 1.5 kW, total 18 meters auger

	5
	Material tower
	1
	tower
	6000
	6000
	
	20 tons material tower

	Feeding system total：
	42000
	
	（RMB）

	three
	Egg collection system

	1
	Egg Picking Machine
	4
	SET
	15000
	60000
	[image: ]
	Made of zinc-aluminum-magnesium, soft egg filter, L-shaped egg claw, cascade egg picker with an egg breaking rate of 2‰, and a motor of 0.75 kW. Speed ​​ratio 1;120

	2
	Egg collection belt
	
	
	
	
	
	Super long and durable imported nylon material

	3
	Egg Pickup Card
	
	
	
	
	
	New Materials

	Egg collection system total：
	60000
	
	（RMB）

	4
	 Manure cleaning system

	1
	Manure cleaning machine host
	4
	set
	22500
	90000
	[image: ]
	The rubber coating of the drum increases the friction between the manure belts, and two manure scrapers are installed. The manure cleaning motor is 1.5 kW, with a speed ratio of 1:120

	2
	Manure cleaning belt
	280
	Group
	
	
	
	Imported polymer material, 1.2mm thick PP tape

	3
	Accessories
	280
	Group
	
	
	
	Baffle, support rod (made of galvanized sheet) lifting lug

	5
	Horizontal and oblique manure transport device
	21
	rice
	450
	9450
	[image: ]
	Each set of horizontal manure cleaning is equipped with a transmission roller, a belt pressing roller, and a tensioning roller. The head is equipped with a manure scraper, and the manure belt support rod is T-shaped, which can transport manure more efficiently.

	Total manure removal system:
	99450
	
	（rmb）

	Total environmental control system and auxiliary equipment：
	
	[image: ]
	（rmb）

	Five
	Temperature control system and auxiliary equipment

	1
	Fan
	18
	tower
	1500
	27000
	[image: ]
	1.4*1.4m push-pull type, stainless steel fan blades, 1.1 kW motor

	2
	Wet curtain
	110
	Square meter
	150
	16500
	
	High permeability, aluminum alloy frame, imported pulp, thickness 15cm

	3
	Wet curtain installation accessories
	1
	Dong
	1500
	1500
	[image: ]
	Water pump. Return pipe, elbow, direct pipe, inlet pipe, etc.

	4
	Deflector plates and accessories
	110
	Square meter
	180
	19800
	
	Electric automatic opening

	5
	linkage
	5
	set
	900
	4500
	[image: ]
	Manual and automatic opening

	6
	Lighting
	6
	set
	1500
	9000
	
	Dedicated lighting lines change light according to time

	
	small window for ventilation
	60
	indivual
	120
	7200
	
	Frame 1.15mm*320mm manual and automatic opening

	7
	
7 Microcomputer Intelligent Environment Control System
Environment Control System
	1
	set
	28000
	24000
	[image: ]
	The entire system of 18 wind turbines (overload, overvoltage, undervoltage, phase loss, inverter failure, line breaks, etc., can be timely alarm, and determine the direction of the fault) cell phone at the same time to receive a 10-inch touch screen, a small window to control outdoor temperature compensation

	Total EMS and ancillary equipment：
	109500
	
	（RMB）

	     VII. Summary of costs
	 Summary of costs

	1
	
	
	

	3
	Total costs：
	658470
	（RMB）

	
	Above quote note:The price of 658470RMB is the factory installed price of all equipment. Does not include invoice, does not include freight, does not include tax, does not include equipment installation costs, customers agree with the initial price, details signed contract negotiation.

	eight
	Equipment Engineering Installation Instructions:

	1
	The above quotation is valid for 15 days. The labor cost for foreign installation guidance is 100 US dollars per person per day.

	2
	The above quotation does not include cables other than equipment, which need to be prepared by customers.

	3
	Before installation, Party B needs to provide an air compressor, and the front and rear ends of the chicken house need to be equipped with power supplies and installation cables。

	4
	If the company needs to arrange the installation, please arrange the accommodation and meals for the installers according to the situation.。

	5
	When installing the equipment, Party B must appoint two full-time personnel to accompany the installation and training to facilitate the normal operation, operation and maintenance of the equipment.

	Nine
	Company address, contact information and service phone number: 008613917849689; Email: landiii@foxmail.com
Whatapp: https://wa.me/13917856548

	1
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